AQ Photo
Film Processing Procedures

Presoak – 1-3 minutes – tap water at 68-70 degrees – agitate continuous 30 sec.

Developer – SEE POSTING - dilution ratio + temperature + film speed = film manufacturers  time recommendations – agitate first 30 sec.  then, 5 sec. of every 30 seconds. 
Rap Tank following each agitation to release air bubbles. 

1 Roll of Kentmere 400 @ 70° = .5ml to 12.5ml    

1 Roll of Ilford HP 5 @ 70 ° = .5ml to 12.5ml 

Stop Bath – Working Solution (DO NOT DILUTE) -  fill tank with stop bath solution or tap water – 15-30 sec. - agitate continuously *RECYCLE

Water rinse - fill tank and empty 1 time. 

Fixer – Working Solution (DO NOT DILUTE) - ( Kentmere and Ilford HP5 5 min. ) - agitate first 30 sec.  then, 5 sec. every 30 sec. *RECYCLE

Water Rinse - 1 min. - continuous agitation

Washing Aid (perma wash) - 1 min. - continuous agitation *RECYCLE

Final Wash – 5 minutes - continuous running water. 

Wetting Agent – (photo-flo) – 30 sec. or double dip and twirl and drain. *RECYCLE

Wipe and Hang 

CLEAN TANKS, TOPS AND REELS WITH WATER AND DRAIN, CLEAN UP ANY SPILLS OR DRIPS AND TURN OFF ANY RUNNING WATER.